**Hints for safe Activation Riddle**

**General:**

Put the switches in the correct Position and divide the Input Voltage to the correct value for activating the safe

**Voltage Divider:**

Try to put the resistors in series and parallel to divide the voltage

Resistors in parallel decrease the resistance while resistors in series increase the overall resistance

Try to use two one kilo ohm resistors and one two kilo ohm resistor